**Soft Electronic Materials for Sustainable Energy & Healthcare Applications**

Prof Ji-Seon Kim

Department of Physics & Centre for Processable Electronics, Imperial College London, UK

(Email: [ji-seon.kim@imperial.ac.uk](mailto:ji-seon.kim@imperial.ac.uk))

Soft electronic materials such as organic and organic/inorganic hybrid (e.g. perovskites) semiconductors have attracted a huge interest for sustainable energy and healthcare applications. These applications include photovoltaics, photodetectors, solar fuel, and biosensors. One of the key challenges for the development of these devices is a fundamental understanding of the semiconductor thin films in terms of their structure-property relationship. Although promising, there is still a lack of clear understanding of the impact of molecular structures on photophysical and electrochemical processes, and device structures on interfacial energetics and properties, which are critical for high-performance devices.

In this talk, I will introduce our recent work in three main research areas. First, I will discuss the importance of molecular design on photostability of organic photovoltaic materials with a particular focus on non-fullerene acceptors. I will show how the conjugated backbone planarity, rigidity, and end groups can alter their photostability and hence OPV/OPD device performance. Second, incorporation of glycol side chains into the polymer backbone has been used to improve charge-carrier mobilities in OFETs, reduce exciton binding energies in OPVs, and enhance hydrogen-evolution efficiencies in photocatalysts. However, it is not clearly understood how the glycol sidechains impact polaron formation in the polymer backbone to bring about these improvements. Here I will introduce our recent work on femtosecond stimulated Raman spectroscopy to probe the structural evolution of the polymers upon photoexcitation and charge formation. Finally, I will briefly discuss the importance of interfacial energetics of perovskite solar cells, to understand how the interface between interlayers and perovskite affects photovoltaic device performance.

Luke, J., et al., (2022) Strong Intermolecular Interactions Induced by High Quadrupole Moments Enable Excellent Photostability of Non‐Fullerene Acceptors for Organic Photovoltaics. *ADVANCED ENERGY MATERIALS*, 2201267. doi:[10.1002/aenm.202201267](http://doi.org/10.1002/aenm.202201267)

Labanti, C., et al., (2022) Light-Intensity Dependent Photoresponse Time of Organic Photodetectors and Its Molecular Origin, *NATURE COMMUNICATIONS*, <https://doi.org/10.1038/s41467-022-31367-4>

Labanti, C., et al., (2021) Selenium-Substituted Non-Fullerene Acceptors: A Route to Superior Operational Stability for Organic Bulk Heterojunction Solar Cells. *ACS NANO*, *15*(4), 7700-7712. doi:[10.1021/acsnano.1c01345](http://doi.org/10.1021/acsnano.1c01345)

Park, S. Y., (2021). Organic Bilayer Photovoltaics for Efficient Indoor Light Harvesting. *ADVANCED ENERGY MATERIALS*, *12*(3), doi:[10.1002/aenm.202103237](http://doi.org/10.1002/aenm.202103237)

Luke, J., et al. (2021). A Commercial Benchmark: Light-Soaking Free, Fully Scalable, Large-Area Organic Solar Cells for Low-Light Applications. *ADVANCED ENERGY MATERIALS*, *11*(9), doi:[10.1002/aenm.202003405](http://doi.org/10.1002/aenm.202003405)

Wu, J., et al. (2020). Exceptionally low charge trapping enables highly efficient organic bulk heterojunction solar cells. *ENERGY & ENVIRONMENTAL SCIENCE*, *13*(8), 2422-2430. doi:[10.1039/d0ee01338b](http://doi.org/10.1039/d0ee01338b)

Tan, E., et al. (2022). The Role of Long-Alkyl-Group Spacers in Glycolated Copolymers for High-Performance Organic Electrochemical Transistors. *ADVANCED MATERIALS*, doi:[10.1002/adma.202202574](http://doi.org/10.1002/adma.202202574)

Limbu, S., et al. (2021). Solid-State Ionic Liquid: Key to Efficient Detection and Discrimination in Organic Semiconductor Gas Sensors. *ACS APPLIED ELECTRONIC MATERIALS*, *3*(5), 2152-2163. doi:[10.1021/acsaelm.1c00157](http://doi.org/10.1021/acsaelm.1c00157)

Chin, Y. -C., et al., (2022). Suppressing PEDOT:PSS Doping-Induced Interfacial Recombination Loss in Perovskite Solar Cells. *ACS ENERGY LETTERS*, *7*(2), 560-568. doi:[10.1021/acsenergylett.1c02577](http://doi.org/10.1021/acsenergylett.1c02577)

Daboczi, M., et al., (2021). Optimal Interfacial Band Bending Achieved by Fine Energy Level Tuning in Mixed-Halide Perovskite Solar Cells. *ACS ENERGY LETTERS*, *6*(11), 3970-3981. doi:[10.1021/acsenergylett.1c02044](http://doi.org/10.1021/acsenergylett.1c02044)

Daboczi, M., et al., (2020). Towards efficient integrated perovskite/organic bulk heterojunction solar cells: interfacial energetic requirement to reduce charge carrier recombination losses. *ADVANCED FUNCTIONAL MATERIALS*, *30*(25), 1-8. doi:[10.1002/adfm.202001482](http://doi.org/10.1002/adfm.202001482)